
Step 1. Please keep the buzzer be turned off, show as the following picture:




Step 2. Upgrade Firmware via mBlock, as follows:



1. Download the latest mBlcok v3.3.2 in this link and decompress it: http://learn.makeblock.com/software/

2. Power off the Orion Board and connect it to PC with USB cable:


3. Install the mBlock software and open it, then choose the**Me Orion** under **Board**:



4.  Choose the correct**Serial port**of Orion Board under **Connect** ->**Serial Port**: (Here my Orion Board's serial port is COM4, and you can check your Orion board serial port under your computer's **Device Manager**->**Ports (COM&LPT)**)

5. Then choose the **Upgrade Firmware** by going to **Connect**->**Upgrade Firmware,**then **Close** when it shows **Upload Finish**.



**Note:** Above Steps take windows PC for example, if your PC is Mac, you need pay attention to two points bellow:

1. Before reset default program, need install a driver for Mac, here is the link to download the driver: <http://blog.sengotta.net/wp-content/uploads/2015/11/CH34x_Install.zip>
2. When choose Serial port under **Connect**->**Serial Port**, please choose **/dev/tty.wchusbserial1410**.