

Step 1: Download the latest mBlock software (V3.3.3) in this link: <http://learn.makeblock.com/software/>

    Decompress the file after download and install mBock software on PC.



Step 2: Use the USB cable connect mBot to PC and power on the mBot.




Step 3: Open mBlock v3.3.3, choose **mBot**under **Board**:



Step 4: Choose the correct Serial Port for mBot under **Connect-**>**Serial Port**: (Here my mBot's serial port is COM3, and you can check your mBot serial port under your computer's **Device Manager**->**Ports (COM&LPT)**)

        Step 5: Go to **Connect**->**Reset Default Program**->**mBot**, wait until it says**Upload Finish**.



Note: Above Steps take windows PC for example, if your PC is Mac, you need pay attention to two points bellow

1. Before reset default program, need install a driver for Mac, here is the link to download the driver:

<http://blog.sengotta.net/wp-content/uploads/2015/11/CH34x_Install.zip>

1. When choose Serial port under **Connect**->**Serial Port**, please choose **/dev/tty.wchusbserial1410**.