


**P**lease kindly test it through home position refer to the following steps:

1. Manually move the carriage to a position (any position where X>0, Y>0).


2. Power on the Laserbot and connect it to PC with USB cable.

3. Upgrade firmware for it with mLaser software refer to following picture.

4.  Reconnect USB cable and connect serial port on mLaser.



5. Go to test if the LaserBot works with home position (refer to steps below):



If the carriage go to Home position (X=0, Y=0) properly, means both the X axis and Y axis are working.