Please be aware that wireless program with 2.4G/Bluetooth connection can only do online debug and you have to be disconnected from 2.4g/Bluetooth and be connected with the USB cable if you are planning on uploading programs to the mBot for standalone operations

The 2.4G/Bluetooth wireless connections allow you to use the mBot firmata to send commands over the air from the computer via Bluetooth or WiFi, but you must have the mBot connected via the USB cable if you wish to upload programs to run unattended on the mBot. The reason is the Bluetooth and WiFi modules cannot use the onboard programmer that is required to load the program into the mBot's memory. When a program is "uploaded" via the USB cable, it overwrites anything else in memory and replaces it with the new program.